


	Tender texts as templates for construction projects in which a tender will be issued

Product:
LIMAFLEX120 –black anodized–
L-Shape
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Limaflex® aluminium path and flower metal edging,
straight shape, deliver and install in accordance with the manufacturer's installation instructions. Flexible special profile black anodized that can be extended using profile connecting elements, with a smooth side and top edge
Item:	Straight with guide mount for 90° retaining anchor
Item no.:	P12E25
Profile height:	120 mm
Length:	2,500 mm
Colour:	black anodised
Item:	Connector for optional connection of the P12N25 profile in the
	upper profile area
Item no.:	V12N10
Length:	100 mm 
Colour:	mill finish, natural aluminium silver-grey
Item:	Profile anchor 90° (also suitable as butt connector) for guide holder
	in path and flower metal edging
Item no.:	PVA40
Profile height:	35 mm
Width:	40 mm
Round hole:	Ø 7.5 mm
Colour:	mill finish, natural silver-grey
Manufacturer:	QualityEdging FZ LLC
	Tel./WhatsApp: +971 50 3464005
	www.qualityedging.com
	E-Mail: sales@qualityedging.com
	Compass Building, Al Shohada Road
	Al Hamra Industrial Zone
	Ras Al Khaimah, United Arab Emirates
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