


	Tender texts as templates for construction projects in which a tender will be issued

Product:
VIAFLEX200
Straight Shape
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Aluminium path and flower bed edging, Viaflex® profile,
straight shape, deliver and install in accordance with the manufacturer's installation instructions. Flexible, interlocking special profile, with a blunt upper edge and wedge-shaped lower edge Profile
type:	Straight with hole punching for anchor/spike
Item no.:	PV20NL25
Profile height:	200 mm
Length:	2,500 mm 
Colour:	natural aluminium silver grey
Item:	Connector for optional connection of the PPV20NL25 profile in the
	upper profile area
Item no.:	V12N10
Length:	100 mm 
Colour:	mill finish, natural aluminium silver-grey

Item:	Butt connector
Item no.:	V15N10
Profile height:	approx. 140 mm (approx. 55 mm lower than the edging profile and therefore 
	barely visible after installation)
Length:	100 mm
Colour:	natural aluminium silver grey
Item:	Anchor/Spike, rounded, upper edge with locking tab, lower edge tapering
	to a point
Item no.:	EN40
Length:	400 mm 
Colour:	natural aluminium silver grey
Manufacturer:	QualityEdging FZ LLC
	Tel./WhatsApp: +971 50 3464005
	www.qualityedging.com
	E-Mail: sales@qualityedging.com
	Compass Building, Al Shohada Road
	Al Hamra Industrial Zone
	Ras Al Khaimah, United Arab Emirates
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